LOG Thr1996 [GasLinkClient_Base.init()] init
LOG Thr1996 [GasLinkClient_Test.init()] constructing GasLinkClient_Test
LOG Thr1996 [GasLinkClient_Test.init()] Logging to : 
e:\temp_build\gas_uber.8.2.202054.source\qgis/AppData\ioGAS.QGIS\plugin.log.txt
LOG Thr1996 [[GasLinkComms.connect()] port=2718] 
LOG Thr1996 [GasLinkComms.connect()] tcp/ip socket initialised
LOG Thr7892 [GasLinkComms.listen()] 
LOG Thr1996 [GLMClient.sendMessage()] init
LOG Thr1996 [] writing to e:\temp_build\gas_uber.8.2.202054.source\qgis/AppData\ioGAS.QGIS\glm.message.temp.txt
LOG Thr1996 [GasLinkComms.sendMessage()] init
LOG Thr1996 [GasLinkComms.sendMessage()] msg Sent
LOG Thr1996 [GLMClient.sendGLMConnect()] GLMConnect Sent, protocol ver:0.2/6
LOG Thr1996 [GLMClient.waitForMessages()] waiting for 3 messages
LOG Thr7892 [GasLinkComms.listen()] got message :
<?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMConnectDone connectionOK="true" ServerVer
Block Count:1
Raised On thread: Thread-10
LOG Thr7892 [TST test_non earth] RX <?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMConnectDone connectionOK="true" ServerVersion="0.2" ServerMinorVersion="6"/>
LOG Thr7892 [TST test_non earth]     calling handler in same thread
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Received msg of type : <class 'gaslink.GLMConnectDone'>
LOG Thr7892 [GLMClient.handle_GLMConnectDone()] 
LOG Thr7892 [TST test_non earth] CONNECTED
LOG Thr7892 [handle_GLMConnectDone] connect done OK, ioGAS is GLM 0.2  6
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Processed : <class 'gaslink.GLMConnectDone'>
LOG Thr7892 [GasLinkComms.listen()] got message :
<?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMSendData stateNull="false" name="gis.smal
Block Count:1
Raised On thread: Thread-10
LOG Thr7892 [TST test_non earth] RX <?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMSendData stateNull="false" name="gis.small.nonearth.gas" newFile="true"><specialColumns><map_east>east</map_east><map_north>north</map_north><map_elevation>RL</map_elevation><map_epsg>0</map_epsg><id>id</id></specialColumns><columns><column><origonalName>id</origonalName><aliasName>id</aliasName><type>Numeric</type></column><column><origonalName>east</origonalName><aliasName>east</aliasName><type>Numeric</type></column><column><origonalN
LOG Thr7892 [TST test_non earth]     calling handler in same thread
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Received msg of type : <class 'gaslink.GLMSendData'>
LOG Thr7892 [GLMClient.handle_GLMSendData()] 
LOG Thr7892 [GLMClient.handle_GLMSendData()] stateNull=False  name =gis.small.nonearth.gas
LOG Thr7892 [GasLinkClient_Test.display_data()] DOING NOTHING
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Processed : <class 'gaslink.GLMSendData'>
LOG Thr7892 [GasLinkComms.listen()] got message :
<?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMSendAttributes><colourAttributes><title>a
Block Count:1
Raised On thread: Thread-10
LOG Thr7892 [TST test_non earth] RX <?xml version="1.0" encoding="UTF-8" standalone="yes"?><GLMSendAttributes><colourAttributes><title>atta</title><colourAttribute><name>Default Colour</name><colour>-16777216</colour><visible>true</visible></colourAttribute><colourAttribute><name>A</name><colour>-65536</colour><visible>true</visible></colourAttribute><colourAttribute><name>B</name><colour>-16711936</colour><visible>true</visible></colourAttribute><colourAttribute><name>C</name><colour>-11028649</colour><visible>true</visible></col
LOG Thr7892 [TST test_non earth]     calling handler in same thread
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Received msg of type : <class 'gaslink.GLMSendAttributes'>
LOG Thr7892 [GLMClient.handle_GLMSendAttributes()] 
LOG Thr7892 [GasData_Link.load_SpecialColumns()] specialColumns.map_epsg found in message:0
LOG Thr7892 [GasData_Link.load_SpecialColumns()] Setting Projection from map_epsg to:0
LOG Thr7892 [GasData_Link.load_data()] all done...
LOG Thr7892 [GasLinkClient_Test.display_data()] DOING NOTHING
LOG Thr7892 [GLMClient_Base.on_message_received()  ] Processed : <class 'gaslink.GLMSendAttributes'>
LOG Thr1996 [GLMClient.waitForMessages()]  - all received
LOG Thr1996 [test_non earth] python client class connected, and (JAVA) SERVER reports gaslink client is QGIS ver 2006
LOG Thr1996 [test_non earth] stopping gas main

LOG Thr7892 [GasLinkComms.listen] STREAM ENDED
LOG Thr7892 [GasLinkComms.listen] connection_lost streamEnd True
LOG Thr7892 [TST test_non earth] CONNECTION LOST
LOG Thr7892 [TST test_non earth]     calling handler in same thread
LOG Thr7892 [GLMClient_Base.on_connection_lost()] CONNECTION LOST
LOG Thr7892 [GasLinkClient_Test.display_data()] DOING NOTHING
